# Summit Station Skiway Report - May 8, 2017

**SKIWAY:**

Use of center skiway is recommended. Rammsonde penetrometer measurements for snow strength taken weekly.

**Markers**: Skiway markers are free of frost/snow.

Thresholds, Midway, 2000’, Taxiway Entrance “A&B” repaired as required and raised to standard height.

30 % of edge markers raised to 5 feet. Average height of unraised markers above snow surface 0” - 6”. A small number are missing/broken.

**Surface Grooming Completed:**

|  |  |  |
| --- | --- | --- |
| **Phase Type:** | **# since last flight period:** | **# since beginning of season:** |
| **Full width Grooming** | 1 | 2 |
| **Centerline** | 2 | 6 |
| **Turnarounds** | 2 | 4 |

* Skiway preparation in accordance with SOP418 - Construction, Surface and Strength Maintenance Procedures for Summit Station Skiway.
* A compaction cycle is scheduled to be completed prior to the start of the next flight period.
* Additional maintenance will be performed prior to flights as weather conditions / drifting dictate.

**TAXIWAY:**

Markers: Blue flags denoting taxiway area have been raised / replaced.

|  |  |  |
| --- | --- | --- |
| **Phase Type:** | **Since last flight period:** | **Since beginning of season:** |
| **Full Width Grooming** | 2 | 3 |

**APPROACH MARKERS:**

Not raised at this time.

**COMMUNICATIONS:**

|  |  |  |
| --- | --- | --- |
| **VHF/AM** | 123.45 MHz Primary | 122.8 MHz Secondary |
| **HF** | 8.093 MHz Primary | 4.753 MHz Secondary |
| **Iridium** | 8816.314.60730 |  |

* Note: - BH Office HF not currently operational

**WEATHER:**

Weather station operational.

Weather observations:

* Begin 3 hours prior to first scheduled offdeck.
* Are transmitted 10 minutes prior to each hour (00:50)
* Continue hourly. Provided more frequently in intermittent conditions or upon request.
* End upon departure of final aircraft from Summit or as directed.
* Updated conditions available upon request during flight operations.