**Frequency Table**

Data transmitted from Tower & Solar Tracker to MSF (Adcon Radio Modem, M433MCPROIP): 433MHz, range 1000m

Data transmitted from NOAA radiometer (on Swiss Fixed-arm rack) to TAWO: 900MHz spread spectrum link Digi Modem

MSF ICECAPS Ka-band radar: Beam pointed vertically, range ~ ? km, ? GHz