# Summit Station Skiway Report

June 25, 2012

**Primary Skiway:**

**Markers:** All markers along the skiway have been replaced and raised to regulation height.

**Surface:**  03 complete grooming phases have been completed since the last flight on June 12, 2012. The skiway was groomed June 18, 2012. Afterwards, approximately 2 inches of drift snow/ falling snow had been deposited on the skiway. The entire skiway was groomed again on June 23 and June 24.

We recommend using the center of the skiway.

The entire skiway is usable.

**Comments:** Rammsonde test last week showed the snow to be soft to quite a depth. We have cooled off a few degrees since earlier in the week, so this may have improved. Skiway is free of wind rows and we don’t think there are any rollers.

**Taxiway:** Markers: Blue flags denoting taxiway area in place.

Surface: 03 complete taxiway phases have been completed since the last the last flight.

**Approach:** All approach flags have been replaced and set at regulation height.

**Comms:** VHF/AM base operating on 123.45MHz (Primary), 122.8MHz (Secondary)

HF base operating on 8.093

IRIDIUM 88-631-460-730

**Weather:** Weather station operating.

Observations begin 3 hours prior to first off deck and continue hourly until last off-deck or as directed. Observations reported daily at 12 GMT.

Updated conditions available upon request during flight operations.

**Other:** Rammsonde penetrometer (snow strength) measurements are ongoing.

High-speed turnarounds at both ends of the skiway have been groomed 03 times since last flight period.