# Summit Station Skiway Report

DATE

**Primary Skiway:**

Markers: All skiway markers have been raised and all damaged markers replaced. (OR CURRENT STATUS)

Surface: XX grooming phases and XX centerline phases have been completed since the last flight period .

XX grooming phases and XX centerline grooming phases have been completed since the beginning of the season.

*Note: A complete grooming phase represents 13 passes for the full length for the skiway.*

*A centerline 60’ grooming phase represents 4 single passes for the full length of the skiway.*

Comments:

The skiway surface is in good shape and free from washboard effects of recent storms.

Long undulations exist.

Use of center skiway recommended.

Skiway surface softens in warm temps and early morning flights are recommended.

**Taxiway:**

Markers: Blue flags denoting taxiway area in place. (comment on current status if needed.)

Surface: XX complete taxiway phases have been completed since the last flight period.

XX complete taxiway phases have been completed since the beginning of the season.

*Note: A complete taxiway grooming phase represents 26 single passes.*

**Approach:**

Markers: Visual verification has been completed and all markers are in place and in good condition.

**Comms:**

VHF/AM base operating on 123.45MHz (Primary), 122.8MHz (Secondary)

HF base operating on 8.093

IRIDIUM 88-631-460-730

**Weather:**

Weather station operating.

Observations begin 3 hours prior to first off deck and continue hourly until last off-deck or as directed. Observations reported daily at 12 GMT.

Updated conditions available upon request during flight operations.

**Other:**

Rammsonde penetrometer (snow strength) measurements are ongoing.

High-speed turnarounds have been groomed at both ends of skiway since last flight period.