**SUMMIT SKIWAY UPDATE 19 APRIL 2017**

**Skiway:**

* Preliminary skiway build in accordance with SOP 418 completed April 7th.
* Skiway sintering for hardness development – April 7th to present.
* Drifting occurred during wind event April 17/18.
* Surface maintenance with Case Tractor and Land Plane will be performed today April 19th per SOP.
* Hardness – see ftp reports

**Markers/Flags:**

* Thresholds 5 x red Raised north and south ends
* Midway 5 x red Raised
* 2000’ 3 x black with ‘2’ Raised
* Edges 3 x black All raised from south end to approx. 3000’
* Approach 4 x black 2 sets at north & south raised
* Taxiway Red flags All in place and raised

**Windsock:** In place

**Fueling System:** In place and tested

**Flight Path Issues**:

* Non-eye-safe laser from MSF - EAST OF STATION MAIN BUILDINGS
* Clean Air Zone - SOUTH OF STATION, TAWO